1. Orig tests (changing Rd, mu)

2. Adding cm grains, changing wall grain size

3. Constraining mdot and using ALMA flux

4. Testing mdot and grains (mm v. cm, eps)

5. Testing mdot and rdisk

Below = Example of decent fit to image, but SED wouldn’t fit ALMA flux.

HD142666_024.pdf