2. Adding cm grains, changing wall grain size

With amaxs = 0.25, comparing amaxb = 1mm (above) v. 1 cm (below)



With amaxs = 1 comparing amaxb = 1mm (above) v. 1 cm (below)



